**2024 PRICING**

**CLEAN, OIL, AND ADJUST (COA) – PARTIAL**

**Partial COA** procedures are for specific areas of need only, and include:

* Play test flute to determine what essential work is required
* Oil buildup removal and fresh oil added
* Spring tension and key heights adjusted as needed
* Minor pad shimming/replacement as needed
* Thoroughly play test and adjust to ensure flute is stable and playing to the highest standard

**CLEAN, OIL, AND ADJUST (COA) - FULL**

Recommended as an annual service, the standard **Full COA** procedures performed are as follows:

* Play test flute to determine all essential work that is required
* Body & mechanism thoroughly cleaned (dent removal if requested, hourly fee applies)
* Complete tarnish removal on body & mechanism
* Oil buildup removal and fresh oil added throughout
* Spring tension adjusted as needed
* Correct and adjust key heights to ensure proper venting
* Pad replacement as needed
* Minor pad shimming as needed
* Headjoint cork replaced
* Thoroughly play test and adjust to ensure flute is stable and playing to the highest standard

| **Instrument Type/Level** | **Partial COA** | **Full COA** | **Pad Replacement** |
| --- | --- | --- | --- |
| **Beginner** | from $125 | from $195 | + $30 per pad |
| **Step-Up/ Intermediate** | from $185 | from $295 | + $30 per pad |
| **Professional** | from $255 | from $395 | + $50 per pad |
| **Handmade Professional** | from $295 | from $445 | + $50 per pad |
| **Turnaround Time Estimate** | 3-5 business days | 5-7 business days | Estimate only |

**OVERHAUL**

Recommended every 5-10 years, the standard **Overhaul** procedures are as follows:

* Replacement of**ALL** soft materials including pads, corks, foams, adjustments (trills and D# replaced as needed)
* Key fit and solder joints are evaluated and corrected (if needed)
* Complete flute cleaning and hand polishing (dent removal by request for additional fee)
* Thoroughly play test and adjust to ensure flute is stable and playing to the highest standard

| **Overhaul Type/Level** | **Overhaul Fee** |
| --- | --- |
| **Student/Step-up** | $600 |
| **Professional (Felt)** | From $1,395 |
| **Professional (Synthetic)** | From $1,595 (add $100 for conversion from felt pads) |
| **Turnaround Time Estimate** | 3-4 Weeks |

**REPAD**

Recommended every 5-10 years for times when the mechanism is in good condition but a considerable number of pads need to be replaced. The standard **Repad** procedures include the **Full COA** services in addition to:

* Replacement of **ALL**pads (occasionally also corks, foams, adjustments)
* Detailed body & mechanism cleaning
* Thoroughly play tested and adjusted to ensure it is stable and playing to the highest standard

| **Repad Type/Level** | **Repad Fee** |
| --- | --- |
| **Beginner (Felt)** | from $795 |
| **Intermediate/Entry Professional (Felt)** | from $895 |
| **Professional/Handmade (Felt)** | from $1,095 |
| **Professional/Handmade (Synthetic)** | from $1,195 (add $100 for conversion from felt pads - overhaul only) |
| **Turnaround Time Estimate** | * 1. Weeks |

Hourly Rate: $110/hour

* Headjoint Cork Replacement
* Soldering
* Dent Removal
* Joint fitting
* Polishing
* Emergency Repairs